2023-01-23
Hall: 1 Booth: 1E16

METPACK

Spray line for closures

Spray line for aluminum and plastic closures for the wine, spirits and beverage industry.

The spray cup printing machines equipped with spray pistols mounted on mobile heads that can cover all shapes, even unusual ones. The closures are conveyed into the cabin mounted on a chain with vertical pins and are presented to the spray pistol. Thanks to a special mechanism, the painting operation is performed only when the chain is stationary. This permits a 30 per cent reduction in paint consumption.

The closures then enter the drying zone, which consists of four consecutive drying lines equipped with infrared heaters positioned above and on either side of the lines. This innovative infrared system reduces drying times and guarantees even, rapid drying.

The paint line has compact dimensions and uses clean energy with reduced environmental impact in terms of emissions and consumption.

General characteristics:
Maximum capsule diameter > 45 millimetre
Minimum capsule diameter > 18 millimetre
Maximum capsule height > 70 millimetre
Minimum capsule height > 18 millimetre
Maximum production rate > 200 p/min

Contact:
OMSO SPA
Ms. Marica Manicardi
Via Adige 11/E
42124 Reggio Emilia
Italy
Fon: +390522382696
Fax: +390522301618
E-Mail: manicardi@omso.it
----------------------------------------