2024-01-11
Hall: 3 Booth: 3C38

IPM ESSEN

FiberCell Batch Mixer

The new FiberCell Batch Mixer is multifunctional with an integrated feeding belt. The FiberCell Batch Mixer has exchangeable wear plates which are easy to replace and easy to handle. The machine is automized with a digital control system and remote access system. The watering unit has a built-in timer where it is easy to set the desired time for watering of the substrate. For the FiberCell Batch Mixer no compressed air is needed which makes the machine more silent.

Growing substrate in containerized nurseries supplies water, oxygen, mineral nutrients, and physical support to the plants. To achieve the characteristics of an ideal substrate for containerized plant production, organic and inorganic components are generally mixed together. Organic components include peat moss and composted organic materials like bark, saw dust, rice husk, coconut husk and sugar cane bagasse. Inorganic components include Perlite, vermiculite, and other inorganic materials like sand, pumice, rock wool and polystyrene flakes. Additives such as slow-release fertilizers or dolomitic lime (for pH correction) can also be added to the mix. Even and homogeneous mixing of these components ensures an increase in seed germination rate, rooting success with cuttings and even development of plants in the nursery, minimizing losses.

Specifications

l Dimensions (L x W x H) milimetre: 2661 x 2718 x 2484
l Weight: 1250 kilogram 
l Hopper capacity: Max 1,5 m3 depending on substate
l Power supply: 3x400v+Neutral+GND 50/60hz
l Power requirement: 5 kW
l Water consumption: 20 liters/minute at 2Ba
Contact:
BCC AB
Mr. Andreas Berner
Profilgatan 15
26135 Landskrona
Sweden
Fon: +46 7053050962
Fax: +46418449922
E-Mail: andreas.berner@bccab.com
----------------------------------------