2022-12-15
Hall: 3 Booth: 3C52

IPM ESSEN

pulsFOG Cold fogger Turbo ULV

The Turbo ULV is a portable AC powered pneumatic cold fogger. Its high performance turbine creates a powerful air stream of up to 50 l/s.

The active solution is atomised into a fine aerosol, which is adjustable from approximately ten to 100 μm depending on the flow rate setting. The precise flow regulation is provided by means of interchangeable nozzles. Chemical resistant materials assure long life and high performance for professional fogging jobs.

• Trouble free and simple operation
• High mobility due to small dimensions, low weight and extended fogging tube
• Detachable solution tank for easy filling and cleaning
• Allows space spray and/or residual applications
• High efficiency air filter protects the motor and internal components
• Sturdy construction for professional use

Technical Data:
Packing dimensions : 59 x 35 x 37 centimtre
Weight : 6,6 kilogram net, 8,3 kilogram gross
Capacity of solution tank : nominal 5 Liter
Power supply: 230 V AC / 50-60 Hz or 110 V AC / 50-60 Hz
Electrical power rating: 1,2 kW
Effective fog throwing range: Up to 25 m
Droplet size dependent on nozzle size used: ten to 100 μm

Contact:
pulsFOG Dr. Stahl & Sohn GmbH
Frau Ingrid Hensler
Abigstr. 8
88662 Überlingen
Germany
Fon: +49755192610
Fax: +497551926161
E-Mail: hensler@pulsfog.com
----------------------------------------