2023-04-06
Hall: 1 Booth: 1C38

METPACK

Fit for the future: save resources with sustainable and safe metal packaging

Henkel Adhesive Technologies will present its range of sustainable and safe packaging solutions. Visitors will get insights into resource-efficient, energy-saving surface treatment solutions, coatings and sealants.

As one of the world’s leading metal pretreatment experts, Henkel Adhesive Technologies has been developing smart packaging solutions for food, beverages and household products for many years. The product portfolio is particularly focused on the aspects of safety and sustainability, avoiding the use of basic substances such as bisphenol A (BPA) and polytetrafluoroethylene (PTFE) for example.
Henkel will also be presenting its Triple Safety program at the world’s leading trade fair for metal packaging. To avoid any risks for users, all substances are subjected to a toxicological assessment and then eliminated if they are proven to be harmful. To this end, Henkel has partnered with Austrian research and testing institute OFI in the field of sealants. During a presentation at the METPACK Conference, Henkel will present a risk assessment of BPA-NI coatings for metal packaging with a focus on the aspect of food contact. Henkel also does not use any chemicals under discussion in its coatings to ensure food safety for humans and animals.

A product highlight for the surface treatment of beverage cans is the new low-temperature cleaner. When used in the beverage can washer, Bonderite C-IC 72000 cleans at a lower temperature of 43 degrees Celsius (110 degrees Fahrenheit) compared to 60 degrees Celsius (140 degrees Fahrenheit) for conventional cleaners. The product series is thus able to reduce natural gas consumption and, in turn, the carbon footprint of the facility. In addition to the energy savings made, it also produces less foam and thus optimizes water consumption.

Contact:
Henkel AG & Co. KG aA
Herr Tobias Laxa
Henkelstr. 67
40589 Düsseldorf
Germany
Fon: +492117978948
E-Mail: tobias.laxa@henkel.com
----------------------------------------