2023-04-02
Hall: 1 Booth: 1D43

METPACK

NewV tin LED: metal decoration printing ink for LED driers

NewV tin LED series is an intensive, highly light-sensitive UV ink for drying with LED UV dryers. The metal decoration printing ink can be used with all standard LED spotlights with a wavelength of 385 to 395 nm.

Due to their special formulation, they offer excellent adhesion, fast and stable ink-water balance, high colour strength, optimal reactivity and excellent properties in further processing.

The range includes process colours, opaque white, gold and silver inks and a spot colour mixing system.

Contact:
hubergroup Deutschland GmbH
Herr Jan Museler
Sonnenallee 1
85551 Kirchheim
Germany
Fon: +498990030
E-Mail: jan.museler@hubergroup.com
----------------------------------------